|  |
| --- |
| Colouring London Building Typology |

The following guide provides some typical exterior characteristics of the buildings associated with each age category that has been set by Colouring London. It is designed to be a guide to help students to enter the data into the correct category. It is not a comprehensive guide to building typologies in London.

|  |  |
| --- | --- |
| **Age category** | **Common exterior features/characteristics** |
|  ≥2000 | Glass, metal, concrete, flat roof, multi-storey, modern. |
|  1980–2000 | Brick, double glazing, apex roof, garage, front garden. |
|  1960–1980 | Brick, cladding (wooden weatherboarding or hanging tiles), double glazing, apex roof, garage, front garden.  |
|  1940–1960 | Brick, rendered, single glazing, small traditional windows. |
|  1920–1940 | Art deco style – lead window frames, decorative glass in front doors. |
|  1900–1920 | Brick, rendered or pebble dashed, single glazing, small traditional windows but more decorative in style than Victorian houses. |
|  1880–1900 | Brick, singe glazing, wooden, sash windows, stained glass in front door windows, apex roof, decorative plaster work. |
|  1860–1880 | Brick, singe glazing, sash windows, apex roof, decorative plaster work. |
|  1840–1860 | Brick, singe glazing, wooden windows, apex roof. Chimneys.Often characterised by the two up, two down terraced housing. |
|  1820–1840 | Brick, singe glazing, wooden windows, apex roof made from slate. |
|  1800–1820 | Brick, singe glazing, lead windows, apex roof, symmetrical designs. |
|  1780–1800 | Brick, singe glazing, lead windows, apex roof, symmetrical designs. |
|  1760–1780 | Stone, timber framed windows, thatched roofs, small windows, low door heights. |
|  1740–1760 | Stone, timber framed windows, thatched roofs, small windows, low door heights. |
|  1720–1740 | Stone, timber framed windows, thatched roofs, small windows, low door heights. |
|  1700–1720 | Stone, timber framed windows, thatched roofs, small windows, low door heights. |
|  1680–1700 | Stone, timber framed windows, thatched roofs, small windows, low door heights. |
|  1660–1680 | Stone or clay, exposed timber frames, timber framed windows, thatched roofs, small windows, low door heights. |
|  <1660 | Stone, timber framed windows, small proportions, low door heights. |

Thanks to Historic England for their contribution to this document, which is provided for educational purposes only. Please visit <https://historicengland.org.uk/> for more detailed guides and information about buildings.